Binary archive of retro pc emulator common source code
								8/10/2017

--- What's this ?

This archive includes the binaries of the emulators listed below:

	ASCII
		yayaMSX1	MSX1 (by Mr.tanam and Mr.umaiboux)
		yayaMSX2	MSX2 (by Mr.tanam and Mr.umaiboux)
		yayaMSX2+	MSX2+ (by Mr.umaiboux)
	BANDAI
		eRX-78		RX-78
	CANON
		eX-07		X-07
	CASIO
		eFP-200		FP-200
		eFP-1100	FP-1100
		ePV-1000	PV-1000
		EmuGaki		PV-2000
	COLECO
		yaCOLECOVISION	ColecoVision
	EPOCH
		eSCV		Super Cassette Vision
	EPSON
		eHC-20		HC-20/HX-20
		eHC-40		HC-40/PX-4
		eHC-80		HC-80/PX-8/Geneva
		eQC-10		QC-10 / QX-10
	FUJITSU
		eFM8		FM-8 (by Mr.Artane.)
		eFM7		FM-7 (by Mr.Artane.)
		eFM77		FM-77 (by Mr.Artane.)
		eFM77AV		FM77AV (by Mr.Artane.)
		eFM77AV40	FM77AV40 (by Mr.Artane.)
		eFM77AV40EX	FM77AV40EX (by Mr.Artane.)
		eFM16pi		FM16pi
		eFMR-30		FMR-30
		eFMR-50		FMR-50
		eFMR-60		FMR-60
		eFMR-70		FMR-70
		eFMR-80		FMR-80
	Gijutsu Hyoron Sha
		eBabbage-2nd	Babbage-2nd
	HITACHI
		eBASICMasterJr	BASIC Master Jr
	Homebrew
		eZ80TVGAME	Homebrew Z80 TV GAME SYSTEM
	IBM Japan Ltd
		eJX		PC/JX
	Japan Electronics College
		eMYCOMZ-80A	MYCOMZ-80A
	MITSUBISHI Electric
		EmuLTI8		MULTI8
	National/Panasonic
		yayaFS-A1	FS-A1 (by Mr.umaiboux)
		eJR-100		JR-100
		eJR-800		JR-800
	NEC
		ePC-2001	PC-2001
		yaPC-6001	PC-6001 (by Mr.tanam)
		yaPC-6201	PC-6001mkII (by Mr.tanam)
		yaPC-6401	PC-6001mkIISR (by Mr.tanam)
		yaPC-6601	PC-6601 (by Mr.tanam)
		yaPC-6801	PC-6601SR (by Mr.tanam)
		ePC-8001mkIISR	PC-8001mkIISR
		ePC-8201	PC-8201/PC-8201A
		ePC-8801MA	PC-8801MA
		ePC-9801	PC-9801
		ePC-9801E	PC-9801E/F/M
		ePC-9801U	PC-9801U
		ePC-9801VF	PC-9801VF
		ePC-9801VM	PC-9801VM
		ePC-9801VX	PC-9801VX
		ePC-98DO	PC-98DO
		ePC-98LT	PC-98LT
		eHANDY98	PC-98HA
		ePC-100		PC-100
		eTK-80BS	TK-80BS / COMPO BS/80
		eTK-85		TK-85
	NEC-HE
		ePCEngine	PC Engine / SuperGrafx + CD-ROM^2
	Nintendo
		eFamilyBASIC	Family BASIC
	Pioneer
		ePX-7		PX-7 (MSX1 + LaserDisc)
	SANYO
		ePHC-20		PHC-20
		ePHC-25		PHC-25
	SEGA
		eSC-3000	SC-3000
		yaGAME GEAR	GAME GEAR (by Mr.tanam)
		yaMASTER SYSTEM	MASTER SYSTEM (by Mr.tanam)
	SEIKO
		eMAP-1010	MAP-1010
	SHARP
		EmuZ-80A	MZ-80A (by Mr.Suga)
		EmuZ-80B	MZ-80B
		EmuZ-80K	MZ-80K/C
		EmuZ-700	MZ-700
		EmuZ-800	MZ-800
		EmuZ-1200	MZ-1200
		EmuZ-1500	MZ-1500
		EmuZ-2200	MZ-2200
		EmuZ-2500	MZ-2500
		EmuZ-2800	MZ-2800
		EmuZ-3500	MZ-3500
		EmuZ-5500	MZ-5500
		EmuZ-6500	MZ-6500
		eSM-B-80TE	SM-B-80TE
		eX1		X1
		eX1twin		X1twin
		eX1turbo	X1turbo
		eX1turboZ	X1turboZ
	Shinko Sangyo
		eYS-6464A	YS-6464A
	SONY
		eSMC-70		SMC-70
		eSMC-777	SMC-777
	SORD
		Emu5		m5
	TOMY
		ePyuTa		PyuTa/PyuTa Jr.
	TOSHIBA
		eEX-80		EX-80
		yayaHX-20+	HX-20 + FDD (by Mr.umaiboux)
		EmuPIA		PASOPIA/PASOPIA5
		EmuPIA7		PASOPIA7
	YAMAHA
		eYIS		YIS
	Yuasa Kyouiku System
		eYALKY		YALKY

These binaries are for Windows XP/Vista/7.
DirectX9 and GDI+ are required.
They are tested on Windows 7 Home Premium with SP1.


--- How to use

Common menus:

Control
	Reset			Reset the virtual machine
	--------
	CPU x1			Set CPU clock multipler
	CPU x2
	CPU x4
	CPU x8
	CPU x16
	Full Speed		Run simulation at full speed
	--------
	Paste			Auto key hitting from the clip board text
	Stop			Stop the auto key hitting
	Romaji to Kana		Enter kana letters with alphabet keys
	--------
	Save State		Save the virtual machine state
	Load State		Load the virtual machine state
	--------
	Debug Main CPU		Open console and debug target CPU like SYMDEB
	Close Debugger		Close debugger console
	--------
	Exit			Terminate the emulator

Cart
	Insert			Insert the cart image
	Eject			Eject the cart image
	--------
	History			Insert the cart image

FD
	Insert			Insert the floppy disk image
	Eject			Eject the floppy disk image
	--------
	Write Protected		Set the write protection of the inserted disk
	Correct Timing		Emulate FDC with correct timing
	Ignore CRC Errors	Ignore crc error status
	----
	History			Insert the floppy disk image

CMT
	Play			Insert the cassette tape image to play
	Rec			Insert the cassette tape image to record
	Eject			Eject the cassette tape image
	--------
	Play Button		Control the cassette tape recorder
	Stop Button
	Fast Foward
	Fast Rewind
	--------
	Waveform Shaper		Enable waveform shaping for *.wav data
	--------
	History			Insert the cassette tape image to play

Device
	Sound
		Sound Device Types
		--------
		Play FDD Noise	Enable playing FDD noise (seek, head up/down)
		Play CMT Noise	Enable playing CMT noise (relay on/off)
		Play CMT Sound	Enable playing CMT signal sound
	Display
		Monitor Types
		--------
		Scanline	Draw scanline

Host
	Rec Movie 60fps		Record the movie to avi and wav files
	Rec Movie 30fps
	Rec Movie 15fps
	Rec Sound		Record the wave file
	Stop			Stop recording
	Capture Screen		Capture the screen to png file
	--------
	Screen
		-
		Window x1	Set the window size
			:
		Window x8
		Fullscreen ?x?	Set the fullscreen size
		--------
		Dot By Dot	Set the stretch screen mode in the fullscreen
		Stretch (Aspect)
		Stretch (Fill)
		--------
		Rotate 0deg	Rotate the screen
		Rotate +90deg
		Rotate 180deg
		Rotate -90deg
	Filter
		RGB Filter	Enable the RGB CRT filter
		None
	Sound
		2000Hz		Set the sound frequency
		4000Hz		You need to restart the emulator
		8000Hz
		11025Hz
		22050Hz
		44100Hz
		48000Hz
		96000Hz
		--------
		50msec		Set the sound buffer size (latency)
		100msec		You need to restart the emulator
		200msec
		300msec
		400msec
		--------
		Realtime Mix	Mix the sound in realtime
		Light Weight Mix
		--------
		Volume		Set the volume of each sound device
	Input
		Joystcik #1/#2	Setup Joystick buttons
	--------
	Use Direct3D9		Enable Direct3D9 to render screen
	Wait Vsync		Wait Vsync when Direct3D9 is enabled
	Use DirectInput		Enable DirectInput for keyboard
	Disable Windows8 DWM	Disable the Desktop Window Manager
	Show Status Bar		Show/Hide the status bar in windwo mode

Accelerator Keys:

	Alt+Enter	Fullscreen
	Ctrl+Enter	Grab the mouse cursor
	Alt+Ctrl+Enter	Run simulation at full speed
	Application	Enter kana letters with alphabet keys


--- Note

For Windows PC environment:

	Support Windows PC compatible mouse and joystick devices.

	Shortcut key:
		ALT+RETURN  - Switch window / fullscreen
		CTRL+RETURN - Swtich enable / disenable the mouse control

	*) While the mouse control is enabled, the mouse cursor is hidden.

Floppy disk images:

	Supoort D88, TeleDisk, ImageDisk, and CPDRead format disk images.

Cassette tape images:

	Support wav files (PCM only) or special format images for each machine.

CD-ROM images:

	Support BIN/IMG+CUE or IMG+CCD (CloneCD) format images.

FDD noise:

	Place the wave files below: FDDSEEK.WAV. HEADDOWN.WAV. HEADUP.WAV

CMT noise:

	Place the wave files below: RELAY_ON.WAV, RELAYOFF.WAV, FAST_FWD.WAV

Save/Load State info:

	The state file contains any disk or other images.
	Please NEVER upload your state files on the web.

	The state file format will be often changed.
	Please don't invite your state file can be loaded after you update
	the emulator binary.


--- Thanks

- vm/datarec.*
	MESS formats/fmsx_cas.c for fMSX cas image decoder
- vm/device.h
	XM6 by Mr.PI.
- vm/fmgen/*
	M88/fmgen by Mr.CISC
- vm/am9511.*
	Xep128 APU core
- vm/disk.*
	TDLZHUF for Teledisk floppy disk image decoder
	MESS formats/dsk_dsk.c for CPDRead floppy disk image decorder
	MESS formats/imd_dsk.c for ImageDisk floppy disk image decorder
- vm/hd44102.*
	MAME HD44102 core and soem modifications by PockEmul
- vm/hd63484.*
	MAME HD63484 core
- vm/huc6280.*
	MESS huc6280 core
- vm/i86.*
	MAME i86 core
- vm/i286.*
	MAME i286 core
- vm/i386.*
	MAME i386 core
- vm/i8259.*
	Neko Project 2 and MESS 8259 core
- vm/ld700.*
	openMSX LD-700
- vm/m6502.*
	MAME m6502 core
- vm/mb8877.*
	XM7 by Mr.PI.
- vm/mc6800.*
	MAME mc6800 core
- vm/mc6809.*
	MAME mc6809 core and improved by Mr.Artane.
- vm/mc6840.*
	MAME Motorola 6840 (PTM) by Mr.James Wallace
- vm/mc6847.*
	MAME mc6847 core
- vm/msm5205.*
	MAME msm5205 core
- vm/mz1p17.*
	MZ-80P3 / MZ-80P4 mode by Mr.Suga
- vm/pc6031.*
	iP6 by Mr.Nishida
- vm/scsi_dev.*
- vm/scsi_host.*
	MAME SCSI bus codes gives me a good hint to implement SCSI protocols
- vm/scsi_cdrom.*
	NEC CD-ROM^2 features by MAME TG16 CD-ROM^2 driver (pce_cdrom.*)
- vm/sn76489an.*
	MAME SN76496 core
- vm/sy6522.*
	MAME Rockwell 6522 VIA by Mr.Peter Trauner and Mr.Mathis Rosenhauer
- vm/t3444a.*
	Mr.Oh!Ishi for the chip specification info
- vm/tf20.*
	vfloppy 1.4 by Mr.Justin Mitchell and Mr.Fred Jan Kraan
	Mr.Fred Han Kraan for EPSON TF-20 hardware design info
- vm/tms3631.*
	Neko Project 2 by Mr.Yui
- vm/tms9918a.*
	MAME TMS9928 core
- vm/tms9995.*
	MAME TMS99xx core
- vm/upd71071.*
	88VA Eternal Grafx by Mr.Shinra
- vm/upd7220.*
	Neko Project 2 by Mr.Yui
- vm/upd765a.*
	M88 fdc/fdu core by Mr.CISC
- vm/upd7752.*
	iP6 by Mr.Nishida
- vm/upd7801.*
	MAME uPD7810 core
	Mr.Komatsu for the chip specification info
- vm/upd7810.*
	MAME uPD7810 core and PockEmul uPD7907 core
- vm/upd16434.*
	PockEmul uPD16434 core
- vm/v99x8.*
	Zodiac V99x8 core, converted to C++ class by Mr.umaiboux
- vm/v9938.*
	MAME V99x8 core, converted to C++ class by Mr.umaiboux
- vm/w3100a.*
	Mr.Oh!Ishi for the chip specification info
- vm/z80.*
	MAME Z80 core
- vm/z80dma.*
	MAME Z80DMA core and improved by Mr.Y.S.
- vm/bmjr/*
	bm2 by Mr.maruhiro
	Mr.Enri for HITACH BASIC Master Jr hardware design info
- vm/colecovision/*
	yaCOLECOVISION by Mr.tanam
- vm/familybasic
	nester by Mr.Darren Ranalli
- vm/fm7/*
	eFM7/77/77AV by Mr.Artane.
- vm/fmr50/bios.*
	FM-TOWNS emulator on bochs
	UNZ pseudo BIOS by Mr.Kasanova
- vm/fp200/*
	PockEmul gives much hints about LCD driver
- vm/gamegear/*
	yaGAMEGEAR/yaMASTERSYSTEM by Mr.tanam
- vm/hc20/*
	Mr.Fred Han Kraan for EPSON HC-20/HX-20 hardware design info
- vm/hc40/*
	Mr.Fred Han Kraan for EPSON HC-40/PX-4 hardware design info
- vm/hc80/*
	Mr.Fred Han Kraan for EPSON HC-80/PX-8/Geneva hardware design info
- vm/hc80/io.*
	Mr.Dennis Heynlein for intelligent ram disk unit
- vm/jr100/*
	Mr.Enri for National JR-100 hardware design info
- vm/jr800/*
	PockEmul JR-800 driver
- vm/m5/*
	MESS sord driver
	Mr.Moriya for Sord M5 hardware design info
- vm/msx/*
	yaMSX1 and yaMSX2 by Mr.tanam
- vm/msx/memory.*
	fMSX Disk BIOS
- vm/mycomz80a/mon/mon.c
	Based on MON80 by Mr.Tesuya Suzuki
- vm/mz80k/memory.*
- vm/mz80k/mz80aif.*
	MZ-80A emulator by Mr.Suga
- vm/mz80k/mz80fio.*
	Mr.Enri for SHARP MZ-80FIO and MZ-80FD hardware design info
- vm/mz80k/printer.*
	The printer interface by Mr.Suga
- vm/mz2500/sasi.*
	X millenium by Mr.Punyu
- vm/mz3500/keyboard.*
	The keycode tables are from Martinuv 8-bitovy blog
	http://www.8bity.cz/2013/adapter-pro-pripojeni-ps2-klavesnice-k-sharp-mz-3500/
- vm/pc6001/*
	yaPC-6001/yaPC-6201/yaPC-6601 by Mr.tanam
- vm/pc8801/pc88.*
	M88 by Mr.CISC
	XM8 by Mr.PI.
	MESS PC-8801 driver
- vm/pc9801/display.*
	Neko Project 2 by Mr.Yui
- vm/pcengine/pce.*
	Ootake (joypad)
	xpce (psg)
	MESS TG16 driver (vdc/vce/vpc/cdrom)
- vm/phc25/*
	PHC-25 emulator by Mr.Tago
- vm/pv1000/*
	Mr.Enri for CASIO PV-1000 hardware design info
- vm/pv2000/*
	Mr.Enri for CASIO PV-2000 hardware design info
- vm/pyuta/*
	MESS tutor driver
	Mr.Enri for TOMY PyuTa Jr. hardware design info
- vm/qc10/*
	Mr.Fred Han Kraan for EPSON QC-10/QX-10 hardware design info
- vm/scv/*
	Mr.Enri and Mr.333 for Epoch Super Cassette Vision hardware info
- vm/x07/io.*
	x07_emul by Mr.Jacques Brigaud
- vm/x1/*
	Many advices by Mr.Y.S.
- vm/x1/psub.*
	X millenium T-tune by Mr.Sato
- vm/x1/display.*
	KANJI ROM support by X1EMU
	X1tuboZ graphic info by Mr.Sato
- vm/yis/*
	YAMAHA provided me some YIS manuals and software disks
	Mr.Moriya analyzed the YIS hardware
- vm/yis/display.*
	KST32B stroke font and its decoder by Mr.Saka.N
- vm/z80tvgame/*
	This homebrew cnosole is designed by Mr.Ishizu
	http://w01.tp1.jp/~a571632211/z80tvgame/index.html
- win32/osd_sound.cpp
	XM7 by Mr.PI. for DirectSound implement
- res/*.ico
	Mr.Temmaru, Mr.Marukun, and Mr.Yoshikun
	See also res/icon.txt

- emulation core design
	nester by Mr.Darren Ranalli
	XM6 by Mr.PI.

----------------------------------------
TAKEDA, toshiya
t-takeda@m1.interq.or.jp
http://takeda-toshiya.my.coocan.jp/
