** UTF-8 **
This is test release for debugging FDC (MB8877).
This contains "Japanese Communication board"(日本語通信カード) emulation.
This also contains UART emulation.
Please check if you have ROM image.
Note:
 Some names of firmwares has changed.
 See fm7.txt and fm77av.txt .
Jan 29, 2018 K.Ohta <whatisthis.sowhat@gmail.com>

Updates:
commit 583d6c628d90055925fa5a7b697a52e60e0052ee
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Mon Jan 29 10:41:33 2018 +0900

    [VM][FM77AV40] Fix FTBFS with Fedora linux.

commit a9157933c5b4761f29290ba7f8aae06f49880156
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Mon Jan 29 10:35:03 2018 +0900

    [VM][MB8877] TRY: Add (temporally) debug log to check DRQ timing for FLEX.
    [VM][MB8877][FM77AV] No need to hack with PSY-O-BLADE.This is test delete.

commit 0a5a54e56ddcca52a239c68d2c3786b388319fe0
Author: K.Ohta <whatisthis.sowhat@gmail.com>
Date:   Mon Jan 29 10:34:25 2018 +0900

    [VM][FM7][DISK] Fix RPM value of 2D/2DD drive to 300rpm.

