| # Compiler Status: Cygwin Run Date: 04:25:47 UTC, Saturday 29 March 2008

## config - config_info - gcc-3.4.4

### Run output:

    GNU C++ version 3.4.4 (cygming special, gdc 0.12, using dmd 0.125)
    Detected Platform: Cygwin
    Boost version 103401

    EXIT STATUS: 0

## audio - ds_enum_test - gcc-3.4.4

### Run output:

    Running 2 test cases...
    The installed DirectSound drivers:
    プライマリ サウンド ドライバ
    Creative Sound Blaster PCI

    The installed DirectSoundCapture drivers:
    プライマリ サウンド キャプチャ ドライバ
    Creative Sound Blaster PCI

    *** No errors detected

    EXIT STATUS: 0

## coroutine - coroutine_test - gcc-3.4.4

### Run output:

    Running 1 test case...
    hello
    hello
    hello

    0
    2
    4
    6
    8
    10
    12
    14
    16
    18

    0
    1
    2
    1
    2
    3
    2
    3
    4

    s00
    s01
    s02
    s10
    s11
    s12
    s20
    s21
    s22

    *** No errors detected

    EXIT STATUS: 0

## coroutine - coro_config_test - gcc-3.4.4

### Run output:

    Running 1 test case...
    use POSIX thread

    *** No errors detected

    EXIT STATUS: 0

## coroutine - generator_test - gcc-3.4.4

### Run output:

    *** No errors detected
    Running 1 test case...
    0
    1
    2
    3
    4
    5
    6
    7
    8
    9

    EXIT STATUS: 0

## coroutine - processor_test - gcc-3.4.4

### Run output:

    Running 1 test case...
    0
    1
    2
    3
    4
    5
    6
    7
    8
    9

    *** No errors detected

    EXIT STATUS: 0

## coroutine - yield_to_arg_test - gcc-3.4.4

### Run output:

    Running 1 test case...
    A(10)
    B(11)

    A(20)
    B(21)
    A(22)

    OK

    *** No errors detected

    EXIT STATUS: 0

## coroutine - yield_to_res_test - gcc-3.4.4

### Run output:

    Running 1 test case...
    A
    B

    A
    B
    A

    A
    B
    C

    OK

    *** No errors detected

    EXIT STATUS: 0

## coroutine - yield_to_test - gcc-3.4.4

### Run output:

    Running 1 test case...
    A
    B

    A
    B
    A

    OK

    *** No errors detected

    EXIT STATUS: 0