# goldfish logcat service:  runs logcat -Q in logd domain

# See global logd.te, these only set for eng & userdebug, allow for all builds

domain_auto_trans(init, logcat_exec, logd)

# Read from logd.
read_logd(logd)

# Write to /dev/ttyS2 and /dev/ttyGF2.
allow logd serial_device:chr_file { write open };
