AVRCP PIXIT for the PTS tool.

PTS version: 6.1

* - different than PTS defaults
& - should be set to IUT Bluetooth address
# - should be set to PTS's bin/audio folder

Required PIXIT settings
-------------------------------------------------------------------------------
Parameter Name			Value
-------------------------------------------------------------------------------
TSPX_security_enabled		FALSE
TSPX_bd_addr_iut		112233445566 (*&)
TSPX_class_of_device		20050C
TSPX_player_feature_bitmask	0000000000000007FFF00070000000000
TSPX_pin_code			0000
TSPX_delete_link_key		FALSE
TSPX_time_guard			300000
TSPX_avrcp_only			FALSE
TSPX_search_string		3
TSPX_max_avc_fragments		10
TSPX_establish_avdtp_stream	TRUE
TSPX_use_implicit_send		TRUE
TSPX_avrcp_version
TSPX_tester_av_role
TSPX_media_directory		C:\Program Files\Bluetooth SIG\Bluetooth PTS\
					bin\audio (#)
TSPX_auth_password		0000
TSPX_auth_user_id		PTS
TSPX_rfcomm_channel		8
TSPX_l2cap_psm			1011
TSPX_no_confirmations		FALSE
TSPX_no_cover_art_folder
TSPX_cover_art_folder
-------------------------------------------------------------------------------
