GATT PICS for the PTS tool.

PTS version: 6.1

* - different than PTS defaults

M - mandatory
O - optional

		Generic Attribute Profile Role
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_GATT_1_1	True		Generic Attribute Profile Client (C.1)
TSPC_GATT_1_2	True		Generic Attribute Profile Server (C.2)
TSPC_GATT_1A_1	True		Complete GATT client (C.3)
TSPC_GATT_1A_2	True		Complete GATT server (C.4)
-------------------------------------------------------------------------------
C.1: Optional to support IF TSPC_GATT_2_2; else IF TSPC_GATT_2_1 it is mandatory
	to support at least one of TSPC_GATT_1_1 OR TSPC_GATT_1_2
C.2: Mandatory to support IF TSPC_GATT_2_2; else IF TSPC_GATT_2_1 it is
	mandatory to support at least one of TSPC_GATT_1_1 OR TSPC_GATT_1_2
C.3: Optional IF TSPC_GATT_1_1 is supported, otherwise Excluded
C.4: Optional IF TSPC_GATT_1_2 is supported, otherwise Excluded
-------------------------------------------------------------------------------


		ATT Bearer Transport
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_GATT_2_1	True		Attribute Protocol Supported over BR/EDR
					(L2CAP fixed channel support) (C.1)
TSPC_GATT_2_2	True		Attribute Protocol Supported over LE (C.2)
-------------------------------------------------------------------------------
C.1: Mandatory IF (SUM ICS 12/2 OR SUM ICS 12/9) is supported, otherwise
	Excluded
C.2: Mandatory IF (SUM ICS 12/7 OR SUM ICS 12/9) is supported, otherwise
	Excluded
-------------------------------------------------------------------------------



		Generic Attribute Profile Support
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_GATT_3_1	True		Client: Exchange MTU (C.2)
TSPC_GATT_3_2	True		Client: Discover All Primary Services (C.1)
TSPC_GATT_3_3	True		Client: Discover Primary Services Service
					UUID (C.1)
TSPC_GATT_3_4	True		Client: Find Included Services (C.1)
TSPC_GATT_3_5	True		Client: Discover All characteristics of a
					Service (C.1)
TSPC_GATT_3_6	True		Client: Discover Characteristics by UUID (C.1)
TSPC_GATT_3_7	True		Client: Discover All Characteristic Descriptors
					(C.1)
TSPC_GATT_3_8	True		Client: Read Characteristic Value (C.1)
TSPC_GATT_3_9	True		Client: Read using Characteristic UUID (C.1)
TSPC_GATT_3_10	True		Client: Read Long Characteristic Values (C.1)
TSPC_GATT_3_11	False (*)	Client: Read Multiple Characteristic
					Values (C.1)
TSPC_GATT_3_12	True		Client: Write without Response (C.1)
TSPC_GATT_3_13	True		Client: Signed Write Without Response (C.1)
TSPC_GATT_3_14	True		Client: Write Characteristic Value (C.1)
TSPC_GATT_3_15	True		Client: Write Long Characteristic Values (C.1)
TSPC_GATT_3_16	True		Client: Characteristic Value Reliable
					Writes (C.1)
TSPC_GATT_3_17	True		Client: Notifications (C.1)
TSPC_GATT_3_18	True		Client: Indications (M)
TSPC_GATT_3_19	True		Client: Read Characteristic Descriptors (C.1)
TSPC_GATT_3_20	True		Client: Read long Characteristic Descriptors
					(C.1)
TSPC_GATT_3_21	True		Client: Write Characteristic Descriptors (C.1)
TSPC_GATT_3_22	True		Client: Write Long Characteristic Descriptors
					(C.1)
TSPC_GATT_3_23	True		Client: Service Changed Characteristic (M)
TSPC_GATT_3B_1	True		Client: Primary Service Declaration (M)
TSPC_GATT_3B_2	True		Client: Secondary Service Declaration (M)
TSPC_GATT_3B_3	True		Client: Include Declaration (M)
TSPC_GATT_3B_4	True		Client: Characteristic Declaration (M)
TSPC_GATT_3B_5	True		Client: Characteristic Value Declaration (M)
TSPC_GATT_3B_6	True		Client: Characteristic Extended Properties (M)
TSPC_GATT_3B_7	True		Client: Characteristic User Description
					Descriptor (M)
TSPC_GATT_3B_8	True		Client: Client Characteristic Configuration
					Descriptor (M)
TSPC_GATT_3B_9	True		Client: Server Characteristic Configuration
					Descriptor (M)
TSPC_GATT_3B_10	True		Client: Characteristic Format Descriptor (M)
TSPC_GATT_3B_11	True		Client: Characteristic Aggregate Format
					Descriptor (M)
TSPC_GATT_3B_12	True		Client: Characteristic Format: Boolean (M)
TSPC_GATT_3B_13	True		Client: Characteristic Format: 2Bit (M)
TSPC_GATT_3B_14	True		Client: Characteristic Format: nibble (M)
TSPC_GATT_3B_15	True		Client: Characteristic Format: Uint8 (M)
TSPC_GATT_3B_16	True		Client: Characteristic Format: Uint12 (M)
TSPC_GATT_3B_17	True		Client: Characteristic Format: Uint16 (M)
TSPC_GATT_3B_18	True		Client: Characteristic Format: Uint24 (M)
TSPC_GATT_3B_19	True		Client: Characteristic Format: Uint32 (M)
TSPC_GATT_3B_20	True		Client: Characteristic Format: Uint48 (M)
TSPC_GATT_3B_21	True		Client: Characteristic Format: Uint64 (M)
TSPC_GATT_3B_22	True		Client: Characteristic Format: Uint128 (M)
TSPC_GATT_3B_23	True		Client: Characteristic Format: Sint8 (M)
TSPC_GATT_3B_24	True		Client: Characteristic Format: Sint12 (M)
TSPC_GATT_3B_25	True		Client: Characteristic Format: Sint16 (M)
TSPC_GATT_3B_26	True		Client: Characteristic Format: Sint24 (M)
TSPC_GATT_3B_27	True		Client: Characteristic Format: Sint32 (M)
TSPC_GATT_3B_28	True		Client: Characteristic Format: Sint48 (M)
TSPC_GATT_3B_29	True		Client: Characteristic Format: Sint64 (M)
TSPC_GATT_3B_30	True		Client: Characteristic Format: Sint128 (M)
TSPC_GATT_3B_31	True		Client: Characteristic Format: Float32 (M)
TSPC_GATT_3B_32	True		Client: Characteristic Format: Float64 (M)
TSPC_GATT_3B_33	True		Client: Characteristic Format: SFLOAT (M)
TSPC_GATT_3B_34	True		Client: Characteristic Format: FLOAT (M)
TSPC_GATT_3B_35	True		Client: Characteristic Format: Duint16 (M)
TSPC_GATT_3B_36	True		Client: Characteristic Format: utf8s (M)
TSPC_GATT_3B_37	True		Client: Characteristic Format: utf16s (M)
TSPC_GATT_3B_38	True		Client: Characteristic Format: struct (M)
-------------------------------------------------------------------------------
C.1: Mandatory IF TSPC_GATT_1_3 is supported, otherwise Optional
C.2: Mandatory IF TSPC_GATT_1_3 AND TSPC_GATT_2_2 is supported, otherwise
	Excluded
-------------------------------------------------------------------------------



		Generic Attribute Profile Support, by Server
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_GATT_4_1	True		Server: Exchange MTU (C.4)
TSPC_GATT_4_2	True		Server: Discover All Primary Services (M)
TSPC_GATT_4_3	True		Server: Discover Primary Services Service
					UUID (M)
TSPC_GATT_4_4	True		Server: Find Included Services (M)
TSPC_GATT_4_5	True		Server: Discover All characteristics of
					a Service (M)
TSPC_GATT_4_6	True		Server: Discover Characteristics by UUID (M)
TSPC_GATT_4_7	True		Server: Discover All Characteristic
					Descriptors (M)
TSPC_GATT_4_8	True		Server: Read Characteristic Value (M)
TSPC_GATT_4_9	True		Server: Read using Characteristic UUID (M)
TSPC_GATT_4_10	True		Server: Read Long Characteristic Values (C.4)
TSPC_GATT_4_11	False (*)	Server: Read Multiple Characteristic
					Values (C.4)
TSPC_GATT_4_12	True		Server: Write without Response (C.2)
TSPC_GATT_4_13	True		Server: Signed Write Without Response (C.4)
TSPC_GATT_4_14	True		Server: Write Characteristic Value (C.3)
TSPC_GATT_4_15	True		Server: Write Long Characteristic Values (C.4)
TSPC_GATT_4_16	True		Server: Characteristic Value Reliable
					Writes (C.4)
TSPC_GATT_4_17	True		Server: Notifications (C.4)
TSPC_GATT_4_18	True		Server: Indications (C.1)
TSPC_GATT_4_19	True		Server: Read Characteristic Descriptors (C.4)
TSPC_GATT_4_20	True		Server: Read long Characteristic
					Descriptors (C.4)
TSPC_GATT_4_21	True		Server: Write Characteristic Descriptors (C.4)
TSPC_GATT_4_22	True		Server: Write Long Characteristic
					Descriptors (C.4)
TSPC_GATT_4_23	True		Server: Service Changed Characteristic (C.1)
-------------------------------------------------------------------------------
C.1: Mandatory IF service definitions on the server can be added, changed, or
	removed, otherwise Optional
C.2: Mandatory IF GATT TSPC_GATT_4_13 is supported, otherwise Optional
C.3: Mandatory IF GATT TSPC_GATT_4_15 is supported, otherwise Optional
C.4: Mandatory IF GATT TSPC_GATT_1_4 is supported, otherwise Optional
-------------------------------------------------------------------------------


		Profile Attribute Types and Characteristic Formats
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_GATT_4B_1	True		Server: Primary Service Declaration (M)
TSPC_GATT_4B_2	True		Server: Secondary Service Declaration (M)
TSPC_GATT_4B_3	True		Server: Include Declaration (M)
TSPC_GATT_4B_4	True		Server: Characteristic Declaration (M)
TSPC_GATT_4B_5	True		Server: Characteristic Value Declaration (M)
TSPC_GATT_4B_6	True		Server: Characteristic Extended Properties (M)
TSPC_GATT_4B_7	True		Server: Characteristic User Description
					Descriptor (M)
TSPC_GATT_4B_8	True		Server: Client Characteristic Configuration
					Descriptor (M)
TSPC_GATT_4B_9	True		Server: Server Characteristic Configuration
					Descriptor (M)
TSPC_GATT_4B_10	True		Server: Characteristic Format Descriptor (M)
TSPC_GATT_4B_11	True		Server: Characteristic Aggregate Format
					Descriptor (M)
TSPC_GATT_4B_12	True		Server: Characteristic Format: Boolean (M)
TSPC_GATT_4B_13	True		Server: Characteristic Format: 2Bit (M)
TSPC_GATT_4B_14	True		Server: Characteristic Format: nibble (M)
TSPC_GATT_4B_15	True		Server: Characteristic Format: Uint8 (M)
TSPC_GATT_4B_16	True		Server: Characteristic Format: Uint12 (M)
TSPC_GATT_4B_17	True		Server: Characteristic Format: Uint16 (M)
TSPC_GATT_4B_18	True		Server: Characteristic Format: Uint24 (M)
TSPC_GATT_4B_19	True		Server: Characteristic Format: Uint32 (M)
TSPC_GATT_4B_20	True		Server: Characteristic Format: Uint48 (M)
TSPC_GATT_4B_21	True		Server: Characteristic Format: Uint64 (M)
TSPC_GATT_4B_22	True		Server: Characteristic Format: Uint128 (M)
TSPC_GATT_4B_23	True		Server: Characteristic Format: Sint8 (M)
TSPC_GATT_4B_24	True		Server: Characteristic Format: Sint12 (M)
TSPC_GATT_4B_25	True		Server: Characteristic Format: Sint16 (M)
TSPC_GATT_4B_26	True		Server: Characteristic Format: Sint24 (M)
TSPC_GATT_4B_27	True		Server: Characteristic Format: Sint32 (M)
TSPC_GATT_4B_28	True		Server: Characteristic Format: Sint48 (M)
TSPC_GATT_4B_29	True		Server: Characteristic Format: Sint64 (M)
TSPC_GATT_4B_30	True		Server: Characteristic Format: Sint128 (M)
TSPC_GATT_4B_31	True		Server: Characteristic Format: Float32 (M)
TSPC_GATT_4B_32	True		Server: Characteristic Format: Float64 (M)
TSPC_GATT_4B_33	True		Server: Characteristic Format: SFLOAT (M)
TSPC_GATT_4B_34	True		Server: Characteristic Format: FLOAT (M)
TSPC_GATT_4B_35	True		Server: Characteristic Format: Duint16 (M)
TSPC_GATT_4B_36	True		Server: Characteristic Format: utf8s (M)
TSPC_GATT_4B_37	True		Server: Characteristic Format: utf16s (M)
TSPC_GATT_4B_38	True		Server: Characteristic Format: struct (M)
-------------------------------------------------------------------------------


		Generic Attribute Profile Service
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_GATT_6_2	True		Discover GATT Services using Service Discovery
					Profile (C.1)
TSPC_GATT_6_3	True		Publish SDP record for GATT services support
					via BR/EDR (C.2)
-------------------------------------------------------------------------------
C.1: Mandatory IF TSPC_GATT_1_1 is supported, otherwise Excluded
C.2: Mandatory IF TSPC_GATT_1_2 is supported, otherwise Excluded
-------------------------------------------------------------------------------


		Attribute Protocol Transport Security
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_GATT_7_1	True		Security Mode 4 (C.1)
TSPC_GATT_7_2	True		LE Security Mode 1 (C.2)
TSPC_GATT_7_3	True		LE Security Mode 2 (C.2)
TSPC_GATT_7_4	True		LE Authentication Procedure (C.2)
TSPC_GATT_7_5	True		LE connection data signing procedure (C.2)
TSPC_GATT_7_6	True		LE Authenticate signed data procedure (C.2)
TSPC_GATT_7_7	True		LE Authorization Procedure (C.2)
-------------------------------------------------------------------------------
C.1: Mandatory IF TSPC_GATT_2_1 is supported, otherwise Excluded
C.2: Optional IF TSPC_GATT_2_2 is supported, otherwise Excluded
-------------------------------------------------------------------------------


		Attribute Protocol Client Messages
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_ATT_3_1	True		Attribute Error Response (M)
TSPC_ATT_3_2	True		Exchange MTU Request (O)
TSPC_ATT_3_4	True		Find Information Request (O)
TSPC_ATT_3_6	True		Find by Type Value Request (O)
TSPC_ATT_3_8	True		Read by Type Request (O)
TSPC_ATT_3_10	True		Read Request (O)
TSPC_ATT_3_12	True		Read Blob Request (O)
TSPC_ATT_3_14	False (*)	Read Multiple Request (O)
TSPC_ATT_3_16	True		Read by Group Type Request (O)
TSPC_ATT_3_17	True		Read by Group Type Response (C.6)
TSPC_ATT_3_18	True		Write Request (O)
TSPC_ATT_3_20	True		Write Command (O)
TSPC_ATT_3_21	True		Signed Write Command (O)
TSPC_ATT_3_22	True		Prepare Write Request (O)
TSPC_ATT_3_24	True		Execute Write Request (C.8)
TSPC_ATT_3_26	True		Handle Value Notification (M)
TSPC_ATT_3_28	True		Handle Value Confirmation (M)
-------------------------------------------------------------------------------
C.6: Mandatory IF TSPC_ATT_3_16 is supported, otherwise Excluded
C.8: Mandatory IF TSPC_ATT_3_22 is supported, otherwise Excluded
-------------------------------------------------------------------------------

		Attribute Protocol Server Messages
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_ATT_4_1	True		Attribute Error Response (M)
TSPC_ATT_4_3	True		Exchange MTU Response (M)
TSPC_ATT_4_5	True		Find Information Response (M)
TSPC_ATT_4_7	True		Find by Type Value Response (M)
TSPC_ATT_4_8	True		Read by Type Request (M)
TSPC_ATT_4_9	True		Read by Type Response (M)
TSPC_ATT_4_11	True		Read Response (M)
TSPC_ATT_4_15	False (*)	Read Multiple Response (C.2)
TSPC_ATT_4_17	True		Read by Group Type Response (M)
TSPC_ATT_4_19	True		Write Response (C.3)
TSPC_ATT_4_20	True		Write Command (O)
TSPC_ATT_4_21	True		Signed Write Command (O)
TSPC_ATT_4_23	True		Prepare Write Response (C.4)
TSPC_ATT_4_25	True		Execute Write Response (C.4)
TSPC_ATT_4_26	True		Handle Value Notification (O)
TSPC_ATT_4_27	True		Handle Value Indication	(O)
-------------------------------------------------------------------------------
C.2: Mandatory IF TSPC_ATT_4_14 is supported, otherwise Excluded
C.3: Mandatory IF TSPC_ATT_4_18 is supported, otherwise Excluded
C.4: Mandatory IF TSPC_ATT_4_22 is supported, otherwise Excluded
C.5: Mandatory IF TSPC_ATT_4_27 is supported, otherwise Excluded
-------------------------------------------------------------------------------


		Attribute Protocol Transport
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_ATT_5_2	True		LE Security Mode 1 (C.2)
TSPC_ATT_5_4	True		LE Authentication Procedure (C.2)
TSPC_ATT_5_7	True		LE Authorization Procedure (C.2)
-------------------------------------------------------------------------------
C.2: Optional to support if 2/2 (Attribute Protocol Supported over LE),
	otherwise Excluded
-------------------------------------------------------------------------------


		Device Configuration
-------------------------------------------------------------------------------
Parameter Name	Selected	Description
-------------------------------------------------------------------------------
TSPC_GAP_0_2	True		LE (C.2)
-------------------------------------------------------------------------------
C.2: Mandatory IF (SUM ICS 34/2 (LE GAP) AND NOT SUM ICS 32/3 (BR/EDR GAP))
	is supported, otherwise Excluded
-------------------------------------------------------------------------------
