
==========================================================================
[Directories]
==========================================================================
common/             Common Files
simple_through/     UZURAフレームワークを使うための最低限必要な初期化が
                    わかるサンプル。
noise_generator/    M系列信号発生器を使ったノイズ発生器。
karaoke_machine/    センター・キャンセル処理でカラオケを生成するサンプル。
                    エフェクトの切り替えやボリューム制御も可能。
ntlogger_example/   Natural Tiny Logger (NT-Logger)のサンプル。
dynamic_menu/       Dynamic Menu Example

==========================================================================
[Terminal #1]
==========================================================================
> sudo /opt/uClinux/bfin-elf/bin/bfin-gdbproxy bfin

Remote proxy for GDB, v0.7.2, Copyright (C) 1999 Quality Quorum Inc.
MSP430 adaption Copyright (C) 2002 Chris Liechti and Steve Underwood
Blackfin adaption Copyright (C) 2008 Analog Devices, Inc.

GDBproxy comes with ABSOLUTELY NO WARRANTY; for details
use `--warranty' option. This is Open Source software. You are
welcome to redistribute it under certain conditions. Use the
'--copying' option for details.

Found USB cable: gnICE+
Connected to libftdi driver.
IR length: 5
Chain length: 1
Device Id: 00100010100000000010000011001011 (0x228020CB)
  Manufacturer: Analog Devices, Inc. (0x0CB)
  Part(0):      BF592 (0x2802)
  Stepping:     2
  Filename:     /opt/uClinux/bfin-elf/bin/../share/urjtag/analog/bf592/bf592
warning:   bfin: no board selected, BF592 is detected
notice:    bfin: jc: waiting on TCP port 2001
notice:    bfin: jc:  (you must connect GDB before using jtag console)
notice:    bfin-gdbproxy: waiting on TCP port 2000

==========================================================================
[Terminal #2]
==========================================================================
> bfin-elf-ldr -T BF592 -c bluetank.ldr bluetank.elf
> bfin-elf-ldr -l bluetank.ldr /dev/ttyUSB0 -b 57600 -C

Creating LDR obj/bluetank.ldr ...
 Adding DXE 'obj/bluetank.elf' ... [jump block to 0xFFA00000] [ELF block: 5768 @ 0xFF800000] [ELF block: 11348 @ 0xFFA00000] OK!
Done!
bfin-elf-ldr -l obj/bluetank.ldr /dev/ttyUSB0 -b 57600 -C
Loading LDR obj/bluetank.ldr ... OK!
Opening /dev/ttyUSB0 ... OK!
Configuring terminal I/O ... OK!
Trying to send autobaud ... OK!
Trying to read autobaud ... OK!
Checking autobaud ... OK!
Autobaud result: 57600bps 36.864mhz (header:0xBF DLL:0x28 DLH:0x00 fin:0x00)
Sending blocks of DXE 1 ... OK!
You may want to run minicom or kermit now
Quick tip: run 'ldr <ldr> <devspec> && minicom'

