/* MANAGED-BY-SYSTEM-BUILDER                                    */
/* VisualDSP++ 5.0 Update 8                                     */
/* LDF Printer version: 5.8.0.3                                 */
/* ldfgen.exe version: 5.8.0.3                                  */
/* VDSG version: 5.8.0.3                                        */

/*
** ADSP-BF506F linker description file generated on Jun 09, 2010 at 22:41:24.
**
** Copyright (C) 2000-2010 Analog Devices Inc., All Rights Reserved.
**
** This file is generated automatically based upon the options selected
** in the LDF Wizard. Changes to the LDF configuration should be made by
** changing the appropriate options rather than editing this file.
**
** Configuration:-
**     crt_doj:                                BF506F_EZKIT_POST_basiccrt.doj
**     processor:                              ADSP-BF506F
**     product_name:                           VisualDSP++ 5.0 Update 8
**     si_revision:                            automatic
**     default_silicon_revision_from_archdef:  0.0
**     using_cplusplus:                        true
**     mem_init:                               false
**     use_vdk:                                false
**     use_eh:                                 true
**     use_argv:                               true
**     running_from_internal_memory:           true
**     user_heap_src_file:                     C:\Build_tools\ant_build\cvsStage\_5.0ExportBlackfinReGen\Examples\Blackfin\Examples\ADSP-BF506F EZ-KIT Lite\Power_On_Self_Test\BF506F_EZKIT_POST_heaptab.c
**     libraries_use_stdlib:                   true
**     libraries_use_fileio_libs:              false
**     libraries_use_ieeefp_emulation_libs:    false
**     libraries_use_eh_enabled_libs:          false
**     system_heap:                            L1
**     system_heap_min_size:                   2k
**     system_stack:                           L1
**     system_stack_min_size:                  2k
**     use_sdram:                              false
**
*/

ARCHITECTURE(ADSP-BF506F)

SEARCH_DIR($ADI_DSP/Blackfin/lib)


// Workarounds are enabled, exceptions are disabled.
#define RT_LIB_NAME(x) lib ## x ## y.dlb
#define RT_LIB_NAME_EH(x) lib ## x ## y.dlb
#define RT_LIB_NAME_MT(x) lib ## x ## y.dlb
#define RT_LIB_NAME_EH_MT(x) lib ## x ## y.dlb
#define RT_OBJ_NAME(x) x ## y.doj
#define RT_OBJ_NAME_MT(x) x ## mty.doj


$LIBRARIES = 

/*$VDSG<insert-user-libraries-at-beginning>                     */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-user-libraries-at-beginning>                     */

   RT_LIB_NAME_MT(small532)
   ,RT_LIB_NAME_MT(io532)
   ,RT_LIB_NAME_MT(c532)
   ,RT_LIB_NAME_MT(event532)
   ,RT_LIB_NAME(ssl506f)
   ,RT_LIB_NAME(drv506f)
   ,RT_LIB_NAME_MT(x532)
   ,RT_LIB_NAME_EH_MT(cpp532)
   ,RT_LIB_NAME_EH_MT(cpprt532)
   ,RT_LIB_NAME(f64ieee532)
   ,RT_LIB_NAME(dsp532)
   ,RT_LIB_NAME(sftflt532)
   ,RT_LIB_NAME(etsi532)
   ,RT_OBJ_NAME_MT(idle532)
   ,RT_LIB_NAME_MT(rt_fileio532)

/*$VDSG<insert-user-libraries-at-end>                           */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-user-libraries-at-end>                           */

   ;

$OBJECTS = 

/*$VDSG<insert-user-objects-at-beginning>                       */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-user-objects-at-beginning>                       */

     RT_LIB_NAME(profile532)
   , $COMMAND_LINE_OBJECTS
   , "cplbtab506f.doj"

/*$VDSG<insert-user-objects-at-end>                             */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-user-objects-at-end>                             */

/*   , RT_OBJ_NAME(crtn506f) */
   ;

$OBJS_LIBS_INTERNAL = 

/*$VDSG<insert-libraries-internal>                              */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-libraries-internal>                              */

   $OBJECTS{prefersMem("internal")}, $LIBRARIES{prefersMem("internal")}

/*$VDSG<insert-libraries-internal-end>                          */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-libraries-internal-end>                          */

   ;

$OBJS_LIBS_NOT_EXTERNAL = 

/*$VDSG<insert-libraries-not-external>                          */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-libraries-not-external>                          */

   $OBJECTS{!prefersMem("external")}, $LIBRARIES{!prefersMem("external")}

/*$VDSG<insert-libraries-not-external-end>                      */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-libraries-not-external-end>                      */

   ;

$OBJS_LIBS_WITH_AUTO_BREAKPOINTS = 

/*$VDSG<insert-libraries-with-auto-breakpoints>                 */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-libraries-with-auto-breakpoints>                 */

   $OBJECTS { FuncName("_main") ||
   FuncName("___lib_prog_term") ||
   FuncName("__primIO") ||
   FuncName("__ov_start") ||
   FuncName("__ov_end") ||
   FuncName("__dbg_assert") ||
   FuncName("__unknown_exception_occurred") ||
   FuncName("_cplb_init") ||
   FuncName("__KernelPanic") },
   $LIBRARIES { FuncName("_main") ||
   FuncName("___lib_prog_term") ||
   FuncName("__primIO") ||
   FuncName("__ov_start") ||
   FuncName("__ov_end") ||
   FuncName("__dbg_assert") ||
   FuncName("__unknown_exception_occurred") ||
   FuncName("_cplb_init") ||
   FuncName("__KernelPanic") }

/*$VDSG<insert-libraries-with-auto-breakpoints-end>             */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-libraries-with-auto-breakpoints-end>             */

   ;

$OBJS_LIBS_WITHOUT_AUTO_BREAKPOINTS = 

/*$VDSG<insert-libraries-without-auto-breakpoints>              */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-libraries-without-auto-breakpoints>              */

   $OBJECTS { !FuncName("_main") &&
   !FuncName("___lib_prog_term") &&
   !FuncName("__primIO") &&
   !FuncName("__ov_start") &&
   !FuncName("__ov_end") &&
   !FuncName("__dbg_assert") &&
   !FuncName("__unknown_exception_occurred") &&
   !FuncName("_cplb_init") &&
   !FuncName("__KernelPanic") },
   $LIBRARIES { !FuncName("_main") &&
   !FuncName("___lib_prog_term") &&
   !FuncName("__primIO") &&
   !FuncName("__ov_start") &&
   !FuncName("__ov_end") &&
   !FuncName("__dbg_assert") &&
   !FuncName("__unknown_exception_occurred") &&
   !FuncName("_cplb_init") &&
   !FuncName("__KernelPanic") }

/*$VDSG<insert-libraries-without-auto-breakpoints-end>          */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-libraries-without-auto-breakpoints-end>          */

   ;


/*$VDSG<insert-user-macros>                                     */
/* Text inserted between these $VDSG comments will be preserved */
/*$VDSG<insert-user-macros>                                     */


/*$VDSG<customize-async-macros>                                 */
/* This code is preserved if the LDF is re-generated.           */


#define ASYNC0_MEMTYPE RAM
#define ASYNC1_MEMTYPE RAM
#define ASYNC2_MEMTYPE RAM
#define ASYNC3_MEMTYPE RAM


/*$VDSG<customize-async-macros>                                 */


MEMORY
{
/*
** ADSP-BF506F MEMORY MAP.
**
** The known memory spaces are as follows:
**
** Internal (core-accessible) memory map:
** =========================================
** 0xFFE00000 - 0xFFFFFFFF  Core MMR registers (2MB)
** 0xFFC00000 - 0xFFDFFFFF  System MMR registers (2MB)
** 0xFFB01000 - 0xFFBFFFFF  Reserved
** 0xFFB00000 - 0xFFB00FFF  Scratch SRAM (4K)
** 0xFFA08000 - 0xFFAFFFFF  Reserved
** 0xFFA04000 - 0xFFA07FFF  L1 instruction SRAM/CACHE (16K)
** 0xFFA00000 - 0xFFA03FFF  L1 instruction Bank A SRAM (16K)
** 0xFF808000 - 0xFF9FFFFF  Reserved
** 0xFF804000 - 0xFF807FFF  L1 Data Bank A SRAM/CACHE (16K)
** 0xFF800000 - 0XFF803FFF  L1 Data Bank A SRAM (16K)
** 0xEF001000 - 0xFF7FFFFF  Reserved
**
** External (interface-accessible) memory map:
** =============================================
** 0xEF000000 - 0xEF000FFF  Boot ROM (4K)
** 0x20400000 - 0xEEFFFFFF  Reserved
** 0x20000000 - 0x203FFFFF  Sync Flash (32M Bits)
** 0x00000000 - 0x1FFFFFFF  Reserved
**
** Notes:
** 0xFF807FEF-0xFF807FFF Required by boot-loader.
*/

   MEM_L1_SCRATCH          { TYPE(RAM) START(0xFFB00000) END(0xFFB00FFF) WIDTH(8) }
   MEM_L1_CODE             { TYPE(RAM) START(0xFFA00000) END(0xFFA07FFF) WIDTH(8) }
   MEM_ARGV                { TYPE(RAM) START(0xFF800000) END(0xFF8000FF) WIDTH(8) }
   MEM_L1_DATA_A           { TYPE(RAM) START(0xFF800100) END(0xFF807FFF) WIDTH(8) }
   MEM_FLASH_BOOT          { TYPE(ASYNC0_MEMTYPE) START(0x20000000) END(0x2001FFFF) WIDTH(8) }
   MEM_FLASH               { TYPE(ASYNC0_MEMTYPE) START(0x20020000) END(0x203FFFFF) WIDTH(8) }
   
   /*$VDSG<insert-new-memory-segments>                          */
   /* Text inserted between these $VDSG comments will be preserved */
   /*$VDSG<insert-new-memory-segments>                          */
   
} /* MEMORY */

PROCESSOR p0
{
   OUTPUT($COMMAND_LINE_OUTPUT_FILE)
   RESOLVE(start, 0xFFA00000)
   RESOLVE(___argv_string, 0xFF800000)
   KEEP(start, _main)
   
   /*$VDSG<insert-user-ldf-commands>                            */
   /* Text inserted between these $VDSG comments will be preserved */
   /*$VDSG<insert-user-ldf-commands>                            */
   
   SECTIONS
   {
      /* Workaround for hardware errata 05-00-0189 and 05-00-0310 -
      ** "Speculative (and fetches made at boundary of reserved memory
      ** space) for instruction or data fetches may cause false
      ** protection exceptions" and "False hardware errors caused by
      ** fetches at the boundary of reserved memory ".
      **
      ** Done by avoiding use of 76 bytes from at the end of blocks
      ** that are adjacent to reserved memory. Workaround is enabled
      ** for appropriate silicon revisions (-si-revision switch).
      */
      RESERVE(___wab0=MEMORY_END(MEM_L1_SCRATCH) - 75, ___l0 = 76)
      RESERVE(___wab2=MEMORY_END(MEM_L1_CODE) - 75, ___l2 = 76)
      RESERVE(___wab4=MEMORY_END(MEM_L1_DATA_A) - 75, ___l4 = 76)
      RESERVE(___wab5=MEMORY_END(MEM_FLASH) - 75, ___l5 = 76)
      
      /*$VDSG<insert-new-sections-at-the-start>                 */
      /* Text inserted between these $VDSG comments will be preserved */
      /*$VDSG<insert-new-sections-at-the-start>                 */
      
      scratchpad NO_INIT
      {
         INPUT_SECTION_ALIGN(4)
         
         /*$VDSG<insert-input-sections-at-the-start-of-scratchpad>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-scratchpad>  */
         
         INPUT_SECTIONS($OBJECTS(L1_scratchpad) $LIBRARIES(L1_scratchpad))
         
         /*$VDSG<insert-input-sections-at-the-end-of-scratchpad>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-end-of-scratchpad>  */
         
      } > MEM_L1_SCRATCH
      
      L1_code
      {
         INPUT_SECTION_ALIGN(4)
         ___l1_code_cache = 0;
         INPUT_SECTIONS($OBJS_LIBS_WITH_AUTO_BREAKPOINTS(program))
         INPUT_SECTIONS($OBJECTS(L1_code) $LIBRARIES(L1_code))
         
         /*$VDSG<insert-input-sections-at-the-start-of-l1_code>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-l1_code>  */
         
         INPUT_SECTIONS($OBJECTS(cplb_code) $LIBRARIES(cplb_code))
         INPUT_SECTIONS($OBJECTS(cplb) $LIBRARIES(cplb))
         INPUT_SECTIONS($OBJECTS(noncache_code) $LIBRARIES(noncache_code))
         INPUT_SECTIONS($OBJS_LIBS_INTERNAL(program))
         INPUT_SECTIONS($OBJS_LIBS_NOT_EXTERNAL(program))
         INPUT_SECTIONS($OBJECTS(program) $LIBRARIES(program))
         
         /*$VDSG<insert-input-sections-at-the-end-of-l1_code>   */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-end-of-l1_code>   */
         
      } > MEM_L1_CODE
      
      L1_data_a_tables
      {
         INPUT_SECTION_ALIGN(4)
         FORCE_CONTIGUITY
         
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a_tables>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a_tables>  */
         
         INPUT_SECTIONS($OBJECTS(ctor) $LIBRARIES(ctor))
         INPUT_SECTIONS($OBJECTS(ctorl) $LIBRARIES(ctorl))
         INPUT_SECTIONS($OBJECTS(.gdt) $LIBRARIES(.gdt))
         INPUT_SECTIONS($OBJECTS(.gdtl) $LIBRARIES(.gdtl))
         
         /*$VDSG<insert-input-sections-at-the-end-of-L1_data_a_tables>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-end-of-L1_data_a_tables>  */
         
      } > MEM_L1_DATA_A
      
      L1_data_a_1
      {
         INPUT_SECTION_ALIGN(4)
         ___l1_data_cache_a = 0;
         INPUT_SECTIONS($OBJECTS(L1_data_a) $LIBRARIES(L1_data_a))
         INPUT_SECTIONS($OBJECTS(L1_data) $LIBRARIES(L1_data))
         
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a_1>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a_1>  */
         
         RESERVE(heaps_and_stack_in_L1_data_a, heaps_and_stack_in_L1_data_a_length = 4096,4)
      } > MEM_L1_DATA_A
      
      L1_data_a_bsz ZERO_INIT
      {
         INPUT_SECTION_ALIGN(4)
         
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a_bsz>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a_bsz>  */
         
         INPUT_SECTIONS( $OBJECTS(L1_bsz) $LIBRARIES(L1_bsz))
         
         /*$VDSG<insert-input-sections-at-the-end-of-L1_data_a_bsz>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-end-of-L1_data_a_bsz>  */
         
      } > MEM_L1_DATA_A
      
      bsz_L1_data_a ZERO_INIT
      {
         INPUT_SECTION_ALIGN(4)
         
         /*$VDSG<insert-input-sections-at-the-start-of-bsz_L1_data_a>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-bsz_L1_data_a>  */
         
         INPUT_SECTIONS($OBJS_LIBS_INTERNAL(bsz))
         INPUT_SECTIONS($OBJS_LIBS_NOT_EXTERNAL(bsz))
         INPUT_SECTIONS($OBJECTS(bsz) $LIBRARIES(bsz))
         
         /*$VDSG<insert-input-sections-at-the-end-of-bsz_L1_data_a>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-end-of-bsz_L1_data_a>  */
         
      } > MEM_L1_DATA_A
      
      L1_data_a
      {
         INPUT_SECTION_ALIGN(4)
         
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a>  */
         
         INPUT_SECTIONS($OBJECTS(voldata) $LIBRARIES(voldata))
         INPUT_SECTIONS($OBJS_LIBS_INTERNAL(data1))
         INPUT_SECTIONS($OBJS_LIBS_NOT_EXTERNAL(data1))
         INPUT_SECTIONS($OBJECTS(data1) $LIBRARIES(data1))
         INPUT_SECTIONS($OBJECTS(constdata) $LIBRARIES(constdata))
         INPUT_SECTIONS($OBJECTS(cplb_data) $LIBRARIES(cplb_data))
         
         /*$VDSG<insert-input-sections-at-the-end-of-L1_data_a>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-end-of-L1_data_a>  */
         
      } > MEM_L1_DATA_A
      
      L1_data_a_2
      {
         INPUT_SECTION_ALIGN(4)
         
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a_2>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-L1_data_a_2>  */
         
         INPUT_SECTIONS($OBJECTS(vtbl) $LIBRARIES(vtbl))
         INPUT_SECTIONS($OBJECTS(.frt) $LIBRARIES(.frt))
         INPUT_SECTIONS($OBJECTS(.rtti) $LIBRARIES(.rtti))
         INPUT_SECTIONS($OBJECTS(.edt) $LIBRARIES(.edt))
         INPUT_SECTIONS($OBJECTS(.cht) $LIBRARIES(.cht))
         
         /*$VDSG<insert-input-sections-at-the-end-of-L1_data_a_2>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-end-of-L1_data_a_2>  */
         
      } > MEM_L1_DATA_A
      
      L1_data_a_stack_heap
      {
         INPUT_SECTION_ALIGN(4)
         RESERVE_EXPAND(heaps_and_stack_in_L1_data_a, heaps_and_stack_in_L1_data_a_length , 0, 4)
         ldf_stack_space = heaps_and_stack_in_L1_data_a;
         ldf_stack_end = (ldf_stack_space + (((heaps_and_stack_in_L1_data_a_length * 2048) / 4096) - 4)) & 0xfffffffc;
         ldf_heap_space = ldf_stack_end + 4;
         ldf_heap_end = (ldf_heap_space + (((heaps_and_stack_in_L1_data_a_length * 2048) / 4096) - 4)) & 0xfffffffc;
         ldf_heap_length = ldf_heap_end - ldf_heap_space;
      } > MEM_L1_DATA_A
      
      FLASH_code
      {
         INPUT_SECTION_ALIGN(4)
         
         /*$VDSG<insert-input-sections-at-the-start-of-FLASH_code>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-FLASH_code>  */
         
         INPUT_SECTIONS($OBJECTS(FLASH_code) $LIBRARIES(FLASH_code))
         INPUT_SECTIONS($OBJS_LIBS_WITHOUT_AUTO_BREAKPOINTS(program))
         
         /*$VDSG<insert-input-sections-at-the-end-of-FLASH_code>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-end-of-FLASH_code>  */
         
      } > MEM_L1_CODE /* MEM_FLASH */
      
      FLASH_constdata
      {
         INPUT_SECTION_ALIGN(4)
         
         /*$VDSG<insert-input-sections-at-the-start-of-FLASH_constdata>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-start-of-FLASH_constdata>  */
         
         INPUT_SECTIONS($OBJECTS(FLASH_data) $LIBRARIES(FLASH_data))
         INPUT_SECTIONS($OBJECTS(constdata) $LIBRARIES(constdata))
         INPUT_SECTIONS($OBJECTS(cplb_data) $LIBRARIES(cplb_data))
         INPUT_SECTIONS($OBJECTS(vtbl) $LIBRARIES(vtbl))
         INPUT_SECTIONS($OBJECTS(.frt) $LIBRARIES(.frt))
         INPUT_SECTIONS($OBJECTS(.rtti) $LIBRARIES(.rtti))
         INPUT_SECTIONS($OBJECTS(.edt) $LIBRARIES(.edt))
         INPUT_SECTIONS($OBJECTS(.cht) $LIBRARIES(.cht))
         
         /*$VDSG<insert-input-sections-at-the-end-of-FLASH_constdata>  */
         /* Text inserted between these $VDSG comments will be preserved */
         /*$VDSG<insert-input-sections-at-the-end-of-FLASH_constdata>  */
         
      } > MEM_L1_CODE /* MEM_FLASH */
      
      
      /*$VDSG<insert-new-sections-at-the-end>                   */
      /* Text inserted between these $VDSG comments will be preserved */
      /*$VDSG<insert-new-sections-at-the-end>                   */
      
   } /* SECTIONS */
} /* p0 */

