[Header]
MagicCookie={0b13fe8c-dfe0-40eb-8900-6712719559a7}
Version=1.0
[File000]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\main.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File001]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\IntQueueTimer.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File002]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\IntQueueTimer_isr.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={92E15EC6-5E91-4BF4-B5FA-C80AD2601AA7}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-ar.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DCFG_INCLUDE_PIC32_ETH_SK_ETH795
TraceCmdString=
DebugOptions=
[File003]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\port.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File004]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\port_asm.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={92E15EC6-5E91-4BF4-B5FA-C80AD2601AA7}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-ar.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DCFG_INCLUDE_PIC32_ETH_SK_ETH795
TraceCmdString=
DebugOptions=
[File005]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\queue.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File006]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\tasks.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File007]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\list.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File008]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\IntQueue.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File009]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\QPeek.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File010]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\lcd.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File011]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\prvTaskTCPIP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File012]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\heap_2.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File013]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\usb_host.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File014]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\usb_config.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File015]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\CustomHTTPApp.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File016]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\usb_host_generic.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File017]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\FSIO.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File018]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\UDP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File019]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\ARP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File020]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\Delay.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File021]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\DHCP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File022]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\DNS.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File023]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\DstaDPlusClientUDP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File024]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\ETHPIC32ExtPhy.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File025]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\ETHPIC32ExtPhyDP83848.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File026]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\ETHPIC32IntMac.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File027]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\FileSystem.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File028]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\FTP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File029]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\Hashes.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File030]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\Helpers.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File031]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\HTTP2.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File032]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\ICMP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File033]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\IP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File034]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\MPFS2.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File035]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\Random.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File036]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\SNTP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File037]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\StackTsk.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File038]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\TCP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File039]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\Tick.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File040]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\MPFSImg2.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File041]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\SD-SPI.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File042]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\prvTaskUSB.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File043]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\prvTaskFS.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File044]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\MACread.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File045]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\SMTP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File046]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\DprsSMTP.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File047]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\serial.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File048]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\serial_isr.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={92E15EC6-5E91-4BF4-B5FA-C80AD2601AA7}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-ar.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DCFG_INCLUDE_PIC32_ETH_SK_ETH795
TraceCmdString=
DebugOptions=
[File049]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\comtest.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File050]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\DHCPs.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File051]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\output\NBNS.o
Folder=Intermediary
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={430F471F-7ECB-4852-A80D-DEF9A5C8E751}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=-DMPLAB_PIC32MX_PORT -DCFG_INCLUDE_PIC32_ETH_SK_ETH795 -DCFG_INCLUDE_UDP_PERF -Wall -fomit-frame-pointer -fschedule-insns -fschedule-insns2
TraceCmdString=
DebugOptions=
[File052]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\.\output\Node.elf
Folder=Output
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={C68E5105-1196-4333-A0BF-3DC57271E614}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-ld.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=--defsym=_min_heap_size=0 --gc-sections -Map="$(BINDIR_)$(TARGETBASE).map" -s -o"$(BINDIR_)$(TARGETBASE).$(TARGETSUFFIX)" -O3
TraceCmdString=
DebugOptions=
[File053]
Location=C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\PIC32MX_MPLAB\.\output\Node.hex
Folder=Output
DeviceName=PIC32MX795F512L
LanguageToolSuiteID={14495C23-81F8-43F3-8A44-859C583D7760}
LanguageToolID={C68E5105-1196-4333-A0BF-3DC57271E614}
LanguageToolLocation=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-ld.exe
PPAD=$(BINDIR)|./output||$(TMPDIR)|./output||$(AINDIR)|..\..\Source\portable\MPLAB\PIC32MX;.||$(INCDIR)|.;.;..\common\include;..\..\source\portable\mplab\pic32mx;..\..\source\include||$(LIBDIR)||$(LKRDIR)||
SOLK=<src>|main.c|IntQueueTimer.c|IntQueueTimer_isr.S|..\..\Source\portable\MPLAB\PIC32MX\port.c|..\..\Source\portable\MPLAB\PIC32MX\port_asm.S|..\..\Source\queue.c|..\..\Source\tasks.c|..\..\Source\list.c|..\Common\Minimal\IntQueue.c|..\Common\Minimal\QPeek.c|lcd.c|prvTaskTCPIP.c|C:\FreeRTOSv7.0.2\Source\portable\MemMang\heap_2.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\usb_host.c|usb_config.c|CustomHTTPApp.c|C:\FreeRTOSv7.0.2\NodeAdapter\Common\USB\Generic Host Driver\usb_host_generic.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\FSIO.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\UDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ARP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Delay.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DNS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DstaDPlusClientUDP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhy.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32ExtPhyDP83848.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ETHPIC32IntMac.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FileSystem.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\FTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Hashes.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Helpers.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\HTTP2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\ICMP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\IP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\MPFS2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Random.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SNTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\StackTsk.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\TCP.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\Tick.c|MPFSImg2.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\SD-SPI.c|prvTaskUSB.c|prvTaskFS.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\MDD File System\MACread.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\SMTP.c|DprsSMTP.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial.c|C:\FreeRTOSv7.0.2_StandAloneNode\Source\serial\serial_isr.S|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\Minimal\comtest.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\DHCPs.c|C:\FreeRTOSv7.0.2_StandAloneNode\NodeAdapter\Common\TCPIP Stack\NBNS.c||<obj>||<lib>||<lkr>|lkd\saap.ld||
SuiteArgsString=
ToolArgsString=--defsym=_min_heap_size=0 --gc-sections -Map="$(BINDIR_)$(TARGETBASE).map" -s -o"$(BINDIR_)$(TARGETBASE).$(TARGETSUFFIX)" -O3
TraceCmdString=
DebugOptions=
[TOOL_LOC_STAMPS]
tool_loc{92E15EC6-5E91-4BF4-B5FA-C80AD2601AA7}=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-ar.exe
tool_loc{430F471F-7ECB-4852-A80D-DEF9A5C8E751}=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-gcc.exe
tool_loc{C68E5105-1196-4333-A0BF-3DC57271E614}=C:\Program Files\Microchip\mplabc32\v2.02\bin\pic32-ld.exe
