Specification link: 11.4 Stroke Properties

painting-stroke-07-t ← index → painting-stroke-09-t

Tests that contain the draft-watermark are under development and may be incorrectly testing a feature.

# painting-stroke-08-t.svg
SVG Image | PNG Image

## Operator Script

## Pass Criteria

There must be no blue bars visible beside the three pink dots. Four semitransparent blue bars, increasingly more opaque, must line up with the yellow dots. Three fully opaque blue bars must line up with the green dots.

## Test Description

Test effects of stroke-opacity range. Values outside the range 0-1.0 must be clamped.

painting-stroke-07-t ← index → painting-stroke-09-t