4.13. Filtering while capturing
Prev | Chapter 4. Capturing Live Network Data | Next

## 4.13. Filtering while capturing

Wireshark uses the libpcap filter language for capture filters. A brief overview of the syntax follows. Complete documentation can be found in the pcap-filter man page. You can find a lot of Capture Filter examples at https://wiki.wireshark.org/CaptureFilters.

You enter the capture filter into the “Filter” field of the Wireshark “Capture Options” dialog box, as shown in Figure 4.3, “The “Capture Options” dialog box”.

A capture filter takes the form of a series of primitive expressions connected by conjunctions (and/or) and optionally preceded by not:

    [not] primitive [and|or [not] primitive ...]

An example is shown in Example 4.1, “A capture filter for telnet that captures traffic to and from a particular host”.

Example 4.1. A capture filter for telnet that captures traffic to and from a particular host

A capture filter for telnet that captures traffic to and from a particular host

    tcp port 23 and host 10.0.0.5

This example captures telnet traffic to and from the host 10.0.0.5, and shows how to use two primitives and the and conjunction. Another example is shown in Example 4.2, “Capturing all telnet traffic not from 10.0.0.5”, and shows how to capture all telnet traffic except that from 10.0.0.5.

Example 4.2. Capturing all telnet traffic not from 10.0.0.5

Capturing all telnet traffic not from 10.0.0.5

    tcp port 23 and not src host 10.0.0.5

A primitive is simply one of the following: [src|dst] host <host>
  This primitive allows you to filter on a host IP address or name. You can optionally precede the primitive with the keyword src|dst to specify that you are only interested in source or destination addresses. If these are not present, packets where the specified address appears as either the source or the destination address will be selected.
ether [src|dst] host <ehost>
  This primitive allows you to filter on Ethernet host addresses. You can optionally include the keyword src|dst between the keywords ether and host to specify that you are only interested in source or destination addresses. If these are not present, packets where the specified address appears in either the source or destination address will be selected.
gateway host <host>
  This primitive allows you to filter on packets that used host as a gateway. That is, where the Ethernet source or destination was host but neither the source nor destination IP address was host.
[src|dst] net <net> [{mask <mask>}|{len <len>}]
  This primitive allows you to filter on network numbers. You can optionally precede this primitive with the keyword src|dst to specify that you are only interested in a source or destination network. If neither of these are present, packets will be selected that have the specified network in either the source or destination address. In addition, you can specify either the netmask or the CIDR prefix for the network if they are different from your own.
[tcp|udp] [src|dst] port <port>

  This primitive allows you to filter on TCP and UDP port numbers. You can optionally precede this primitive with the keywords src|dst and tcp|udp which allow you to specify that you are only interested in source or destination ports and TCP or UDP packets respectively. The keywords tcp|udp must appear before src|dst.

  If these are not specified, packets will be selected for both the TCP and UDP protocols and when the specified address appears in either the source or destination port field.

less|greater <length>
  This primitive allows you to filter on packets whose length was less than or equal to the specified length, or greater than or equal to the specified length, respectively.
ip|ether proto <protocol>
  This primitive allows you to filter on the specified protocol at either the Ethernet layer or the IP layer.
ether|ip broadcast|multicast
  This primitive allows you to filter on either Ethernet or IP broadcasts or multicasts.
<expr> relop <expr>
  This primitive allows you to create complex filter expressions that select bytes or ranges of bytes in packets. Please see the pcap-filter man page at http://www.tcpdump.org/manpages/pcap-filter.7.html for more details.

### 4.13.1. Automatic Remote Traffic Filtering

If Wireshark is running remotely (using e.g. SSH, an exported X11 window, a terminal server, …​), the remote content has to be transported over the network, adding a lot of (usually unimportant) packets to the actually interesting traffic.

To avoid this, Wireshark tries to figure out if it’s remotely connected (by looking at some specific environment variables) and automatically creates a capture filter that matches aspects of the connection.

The following environment variables are analyzed:

SSH_CONNECTION (ssh)
  <remote IP> <remote port> <local IP> <local port>
SSH_CLIENT (ssh)
  <remote IP> <remote port> <local port>
REMOTEHOST (tcsh, others?)
  <remote name>
DISPLAY (x11)
  [remote name]:<display num>
SESSIONNAME (terminal server)
  <remote name>

On Windows it asks the operating system if it’s running in a Remote Desktop Services environment.

### 4.13.2. Stop the running capture

A running capture session will be stopped in one of the following ways:

1. Using the Stop button from the “Capture Info” dialog box.

| Note
The “Capture Info” dialog box might be hidden if the “Hide capture info dialog” option is used.

1. Using the Capture → Stop menu item.
2. Using the Stop toolbar button.
3. Pressing Ctrl+E.
4. The capture will be automatically stopped if one of the Stop Conditions is met, e.g. the maximum amount of data was captured.

### 4.13.3. Restart a running capture

A running capture session can be restarted with the same capture options as the last time, this will remove all packets previously captured. This can be useful, if some uninteresting packets are captured and there’s no need to keep them.

Restart is a convenience function and equivalent to a capture stop following by an immediate capture start. A restart can be triggered in one of the following ways:

1. Using the Capture → Restart menu item.
2. Using the Restart toolbar button.

Prev | Up | Next
4.12. Link-layer header type | Home | Chapter 5. File Input, Output, and Printing