# The Mesa 3D Graphics Library

# Environment Variables

Normally, no environment variables need to be set. Most of the environment variables used by Mesa/Gallium are for debugging purposes, but they can sometimes be useful for debugging end-user issues.

## LibGL environment variables

- LIBGL_DEBUG - If defined debug information will be printed to stderr. If set to 'verbose' additional information will be printed.
- LIBGL_DRIVERS_PATH - colon-separated list of paths to search for DRI drivers
- LIBGL_ALWAYS_INDIRECT - forces an indirect rendering context/connection.
- LIBGL_ALWAYS_SOFTWARE - if set, always use software rendering
- LIBGL_NO_DRAWARRAYS - if set do not use DrawArrays GLX protocol (for debugging)
- LIBGL_SHOW_FPS - print framerate to stdout based on the number of glXSwapBuffers calls per second.
- LIBGL_DRI3_DISABLE - disable DRI3 if set (the value does not matter)

## Core Mesa environment variables

- MESA_NO_ASM - if set, disables all assembly language optimizations
- MESA_NO_MMX - if set, disables Intel MMX optimizations
- MESA_NO_3DNOW - if set, disables AMD 3DNow! optimizations
- MESA_NO_SSE - if set, disables Intel SSE optimizations
- MESA_DEBUG - if set, error messages are printed to stderr. For example, if the application generates a GL_INVALID_ENUM error, a corresponding error message indicating where the error occurred, and possibly why, will be printed to stderr.
  For release builds, MESA_DEBUG defaults to off (no debug output). MESA_DEBUG accepts the following comma-separated list of named flags, which adds extra behaviour to just set MESA_DEBUG=1:
  - silent - turn off debug messages. Only useful for debug builds.
  - flush - flush after each drawing command
  - incomplete_tex - extra debug messages when a texture is incomplete
  - incomplete_fbo - extra debug messages when a fbo is incomplete
  - context - create a debug context (see GLX_CONTEXT_DEBUG_BIT_ARB) and print error and performance messages to stderr (or MESA_LOG_FILE).
- MESA_LOG_FILE - specifies a file name for logging all errors, warnings, etc., rather than stderr
- MESA_TEX_PROG - if set, implement conventional texture env modes with fragment programs (intended for developers only)
- MESA_TNL_PROG - if set, implement conventional vertex transformation operations with vertex programs (intended for developers only). Setting this variable automatically sets the MESA_TEX_PROG variable as well.
- MESA_EXTENSION_OVERRIDE - can be used to enable/disable extensions. A value such as "GL_EXT_foo -GL_EXT_bar" will enable the GL_EXT_foo extension and disable the GL_EXT_bar extension.
- MESA_EXTENSION_MAX_YEAR - The GL_EXTENSIONS string returned by Mesa is sorted by extension year. If this variable is set to year X, only extensions defined on or before year X will be reported. This is to work-around a bug in some games where the extension string is copied into a fixed-size buffer without truncating. If the extension string is too long, the buffer overrun can cause the game to crash. This is a work-around for that.
- MESA_GL_VERSION_OVERRIDE - changes the value returned by glGetString(GL_VERSION) and possibly the GL API type.
  - The format should be MAJOR.MINOR[FC]
  - FC is an optional suffix that indicates a forward compatible context. This is only valid for versions >= 3.0.
  - GL versions < 3.0 are set to a compatibility (non-Core) profile
  - GL versions = 3.0, see below
  - GL versions > 3.0 are set to a Core profile
  - Examples: 2.1, 3.0, 3.0FC, 3.1, 3.1FC
    - 2.1 - select a compatibility (non-Core) profile with GL version 2.1
    - 3.0 - select a compatibility (non-Core) profile with GL version 3.0
    - 3.0FC - select a Core+Forward Compatible profile with GL version 3.0
    - 3.1 - select a Core profile with GL version 3.1
    - 3.1FC - select a Core+Forward Compatible profile with GL version 3.1
  - Mesa may not really implement all the features of the given version. (for developers only)
- MESA_GLES_VERSION_OVERRIDE - changes the value returned by glGetString(GL_VERSION) for OpenGL ES.
  - The format should be MAJOR.MINOR
  - Examples: 2.0, 3.0, 3.1
  - Mesa may not really implement all the features of the given version. (for developers only)
- MESA_GLSL_VERSION_OVERRIDE - changes the value returned by glGetString(GL_SHADING_LANGUAGE_VERSION). Valid values are integers, such as "130". Mesa will not really implement all the features of the given language version if it's higher than what's normally reported. (for developers only)
- MESA_GLSL - shading language compiler options
- MESA_NO_MINMAX_CACHE - when set, the minmax index cache is globally disabled.

## Mesa Xlib driver environment variables

The following are only applicable to the Mesa Xlib software driver. See the Xlib software driver page for details.

- MESA_RGB_VISUAL - specifies the X visual and depth for RGB mode
- MESA_CI_VISUAL - specifies the X visual and depth for CI mode
- MESA_BACK_BUFFER - specifies how to implement the back color buffer, either "pixmap" or "ximage"
- MESA_GAMMA - gamma correction coefficients for red, green, blue channels
- MESA_XSYNC - enable synchronous X behavior (for debugging only)
- MESA_GLX_FORCE_CI - if set, force GLX to treat 8bpp visuals as CI visuals
- MESA_GLX_FORCE_ALPHA - if set, forces RGB windows to have an alpha channel.
- MESA_GLX_DEPTH_BITS - specifies default number of bits for depth buffer.
- MESA_GLX_ALPHA_BITS - specifies default number of bits for alpha channel.

## i945/i965 driver environment variables (non-Gallium)

- INTEL_NO_HW - if set to 1, prevents batches from being submitted to the hardware. This is useful for debugging hangs, etc.
- INTEL_DEBUG - a comma-separated list of named flags, which do various things:
  - tex - emit messages about textures.
  - state - emit messages about state flag tracking
  - blit - emit messages about blit operations
  - miptree - emit messages about miptrees
  - perf - emit messages about performance issues
  - perfmon - emit messages about AMD_performance_monitor
  - bat - emit batch information
  - pix - emit messages about pixel operations
  - buf - emit messages about buffer objects
  - fbo - emit messages about framebuffers
  - fs - dump shader assembly for fragment shaders
  - gs - dump shader assembly for geometry shaders
  - sync - after sending each batch, emit a message and wait for that batch to finish rendering
  - prim - emit messages about drawing primitives
  - vert - emit messages about vertex assembly
  - dri - emit messages about the DRI interface
  - sf - emit messages about the strips & fans unit (for old gens, includes the SF program)
  - stats - enable statistics counters. you probably actually want perfmon or intel_gpu_top instead.
  - urb - emit messages about URB setup
  - vs - dump shader assembly for vertex shaders
  - clip - emit messages about the clip unit (for old gens, includes the CLIP program)
  - aub - dump batches into an AUB trace for use with simulation tools
  - shader_time - record how much GPU time is spent in each shader
  - no16 - suppress generation of 16-wide fragment shaders. useful for debugging broken shaders
  - blorp - emit messages about the blorp operations (blits & clears)
  - nodualobj - suppress generation of dual-object geometry shader code
  - optimizer - dump shader assembly to files at each optimization pass and iteration that make progress
  - ann - annotate IR in assembly dumps
  - no8 - don't generate SIMD8 fragment shader
  - vec4 - force vec4 mode in vertex shader
  - spill_fs - force spilling of all registers in the scalar backend (useful to debug spilling code)
  - spill_vec4 - force spilling of all registers in the vec4 backend (useful to debug spilling code)
  - cs - dump shader assembly for compute shaders
  - hex - print instruction hex dump with the disassembly
  - nocompact - disable instruction compaction
  - tcs - dump shader assembly for tessellation control shaders
  - tes - dump shader assembly for tessellation evaluation shaders
  - l3 - emit messages about the new L3 state during transitions
  - do32 - generate compute shader SIMD32 programs even if workgroup size doesn't exceed the SIMD16 limit
  - norbc - disable single sampled render buffer compression
- INTEL_PRECISE_TRIG - if set to 1, true or yes, then the driver prefers accuracy over performance in trig functions.

## Radeon driver environment variables (radeon, r200, and r300g)

- RADEON_NO_TCL - if set, disable hardware-accelerated Transform/Clip/Lighting.

## EGL environment variables

Mesa EGL supports different sets of environment variables. See the Mesa EGL page for the details.

## Gallium environment variables

- GALLIUM_HUD - draws various information on the screen, like framerate, cpu load, driver statistics, performance counters, etc. Set GALLIUM_HUD=help and run e.g. glxgears for more info.
- GALLIUM_HUD_PERIOD - sets the hud update rate in seconds (float). Use zero to update every frame. The default period is 1/2 second.
- GALLIUM_HUD_VISIBLE - control default visibility, defaults to true.
- GALLIUM_HUD_TOGGLE_SIGNAL - toggle visibility via user specified signal. Especially useful to toggle hud at specific points of application and disable for unencumbered viewing the rest of the time. For example, set GALLIUM_HUD_VISIBLE to false and GALLIUM_HUD_TOGGLE_SIGNAL to 10 (SIGUSR1). Use kill -10 to toggle the hud as desired.
- GALLIUM_HUD_DUMP_DIR - specifies a directory for writing the displayed hud values into files.
- GALLIUM_DRIVER - useful in combination with LIBGL_ALWAYS_SOFTWARE=1 for choosing one of the software renderers "softpipe", "llvmpipe" or "swr".
- GALLIUM_LOG_FILE - specifies a file for logging all errors, warnings, etc. rather than stderr.
- GALLIUM_PRINT_OPTIONS - if non-zero, print all the Gallium environment variables which are used, and their current values.
- GALLIUM_DUMP_CPU - if non-zero, print information about the CPU on start-up
- TGSI_PRINT_SANITY - if set, do extra sanity checking on TGSI shaders and print any errors to stderr.
- DRAW_FSE - ???
- DRAW_NO_FSE - ???
- DRAW_USE_LLVM - if set to zero, the draw module will not use LLVM to execute shaders, vertex fetch, etc.
- ST_DEBUG - controls debug output from the Mesa/Gallium state tracker. Setting to "tgsi", for example, will print all the TGSI shaders. See src/mesa/state_tracker/st_debug.c for other options.

### Clover state tracker environment variables

- CLOVER_EXTRA_BUILD_OPTIONS - allows specifying additional compiler and linker options. Specified options are appended after the options set by the OpenCL program in clBuildProgram.
- CLOVER_EXTRA_COMPILE_OPTIONS - allows specifying additional compiler options. Specified options are appended after the options set by the OpenCL program in clCompileProgram.
- CLOVER_EXTRA_LINK_OPTIONS - allows specifying additional linker options. Specified options are appended after the options set by the OpenCL program in clLinkProgram.

### Softpipe driver environment variables

- SOFTPIPE_DUMP_FS - if set, the softpipe driver will print fragment shaders to stderr
- SOFTPIPE_DUMP_GS - if set, the softpipe driver will print geometry shaders to stderr
- SOFTPIPE_NO_RAST - if set, rasterization is no-op'd. For profiling purposes.
- SOFTPIPE_USE_LLVM - if set, the softpipe driver will try to use LLVM JIT for vertex shading processing.

### LLVMpipe driver environment variables

- LP_NO_RAST - if set LLVMpipe will no-op rasterization
- LP_DEBUG - a comma-separated list of debug options is accepted. See the source code for details.
- LP_PERF - a comma-separated list of options to selectively no-op various parts of the driver. See the source code for details.
- LP_NUM_THREADS - an integer indicating how many threads to use for rendering. Zero turns off threading completely. The default value is the number of CPU cores present.

### VMware SVGA driver environment variables

- SVGA_FORCE_SWTNL - force use of software vertex transformation
- SVGA_NO_SWTNL - don't allow software vertex transformation fallbacks (will often result in incorrect rendering).
- SVGA_DEBUG - for dumping shaders, constant buffers, etc. See the code for details.
- See the driver code for other, lesser-used variables.

### VA-API state tracker environment variables

- VAAPI_MPEG4_ENABLED - enable MPEG4 for VA-API, disabled by default.

### VC4 driver environment variables

- VC4_DEBUG - a comma-separated list of named flags, which do various things:
  - cl - dump command list during creation
  - qpu - dump generated QPU instructions
  - qir - dump QPU IR during program compile
  - nir - dump NIR during program compile
  - tgsi - dump TGSI during program compile
  - shaderdb - dump program compile information for shader-db analysis
  - perf - print during performance-related events
  - norast - skip actual hardware execution of commands
  - always_flush - flush after each draw call
  - always_sync - wait for finish after each flush
  - dump - write a GPU command stream trace file (VC4 simulator only)

Other Gallium drivers have their own environment variables. These may change frequently so the source code should be consulted for details.