"eSCV" - EPOCH Super Cassette Vision Emulator for Win32
								1/5/2008

--- Internal ROM image

	BIOS.ROM	$0000-$0FFF

--- Cart ROM images

	Cart ROM image header:

		db id[4]	'SCV^Z' (53h,43h,56h,1ah)
		db ctype	0 = 16KB, 32KB, 32KB + 8KB
				1 = 32KB + 8KB SRAM
				2 = 32KB + 32KB, 32KB + 32KB + 32KB + 32KB
		db reserver[11]

		(note: if no header, it is recognized that ctype must be 0)

	ctype = 0
		* Standard cart
			16KB ($8000-$BFFF)
		* Milky Princess
		* Super Sansu-puter
			32KB ($8000-$FFFF)
		* Mappy
			32KB (PC5=1, $8000-$FFFF)
		* Nekketsu Kung-fu Road
		* Star Speeder
			32KB (PC5=0, $8000-$FFFF) + 
			8KB (PC5=1, $e000-$FFFF)

	ctype = 1
		* BASIC Nyu-mon
		* Dragon Slayer
		* Pop & Chips
		* Shogi Nyumon
			32KB (PC5=0, $8000-$FFFF) + 
			8KB SRAM

	ctype = 2
		* Doraemon
		* Sky Kid
			32KB (PC5=0, $8000-$FFFF) + 
			32KB (PC5=1, $8000-$FFFF)
		* Dragon Dai Hikyou
			32KB (PC5=0/1 PC6=0, $8000-$FFFF) +
			32KB (PC5=0/1 PC6=0, $8000-$FFFF) +
			32KB (PC5=0 PC6=1, $8000-$FFFF) +
			32KB (PC5=1 PC6=1, $8000-$FFFF)
		* Pole Position 2 (?)
		* Rantou Prowres
		* Waiwai(Y2) Monster Land
			32KB (PC5=0 PC6=0, $8000-$FFFF) +
			32KB (PC5=1 PC6=0, $8000-$FFFF) +
			32KB (PC5=0 PC6=1, $8000-$FFFF) +
			32KB (PC5=1 PC6=1, $8000-$FFFF)

--- Key maps

	Virtual		PC
	--------------------------------
	Joystick-1
	  Directions	Cursor
	  Trigger-1	Z
	  Trigger-2	X
	0-9		0-9
	EN		Enter
	CL		BackSpace
	PAUSE		Space

----------------------------------------
TAKEDA, toshiya
t-takeda@m1.interq.or.jp
http://homepage3.nifty.com/takeda-toshiya/
