# Fluoride 1.0

Declaration ID: [D0026807](https://www.bluetooth.org/tpg/QLI_viewQDL.cfm?qid=26807)  
Qualified Design ID: 67282

Protocol / Profile | Version | Roles
-------------------+---------+-------
L2CAP              | 4.2     | Initiator, Acceptor, LE Master, LE Slave
SDP                | 4.2     | Server, Client
GAP                | 4.2     | BR/EDR, LE Central, LE Periperhal, LE Observer, LE Broadcaster
GATT               | 4.2     | Client, Server; LE and BR/EDR
ATT                | 4.2     | Client, Server; LE and BR/EDR
SM                 | 4.2     | Master (Initiator), Slave (Responder)
AVCTP              | 1.4     | Controller, Target
AVDTP              | 1.2     | Source, Initiator, Acceptor
BNEP               | 1.0     |
GAVDP              | 1.2     | Initiator, Acceptor
MCAP               | 1.0     | Sink
RFCOMM             | 1.2     |
SPP                | 1.2     | A, B
